{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-L"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35L2V1B","FCQG50FVEB / RXS50L2V1B","FCQG60FVEB / RXS60L2V1B"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.7","1.7"]
["","Maks.","","kW","4.0","5.3","5.7"]
["","Nom.","","kW","3.4","5.0","5.7"]
["Cevne spojnice","Tečnost","SP","mm","6.35","6.35","6.35"]
["","Gas","SP","mm","9.5","12.70","12.70"]
["","Ispusni otvor","OD","mm","VP25 (Spoljni preč.32, unutrašnji preč. 25)","VP25 (Spoljni preč.32, unutrašnji preč. 25)","VP25 (Spoljni preč.32, unutrašnji preč. 25)"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","475","705","820"]
["","EER","","","3.58","3.55","3.48"]
["","COP","","","3.50","3.7","3.52"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A"]
["","","Grejanje","","B","A","B"]
["Kapacitet grejanja","Nom.","","kW","4.20","6.00","7.0"]
["","Min.","","kW","1.3","1.7","1.7"]
["","Maks.","","kW","5.2","6.0","7.0"]
["Beleške","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","(4) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(4) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(4) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(5) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(5) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(5) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]