{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35L3V1B"]
["Kapacitet hlađenja","Min.","","kW","1.3"]
["","Maks.","","kW","4.0"]
["","Nom.","","kW","3.4 (2)"]
["Cevne spojnice","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","9.5"]
["","Ispusni otvor","OD","mm","VP25 (Spoljni preč.32, unutrašnji preč. 25)"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","455"]
["","EER","","","3.74 (1)"]
["","COP","","","3.50 (1)"]
["","Direktiva o energetskom označavanju","Hlađenje","","A"]
["","","Grejanje","","B"]
["Kapacitet grejanja","Nom.","","kW","4.20 (2)"]
["","Min.","","kW","1.3"]
["","Maks.","","kW","5.2"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]
["","","","","(3) - 220V"]
["","","","","(4) - 230V"]
["","","","","(5) - 240V"]