{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZASG-MY"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZASG125MUY"]
["Kapacitet hlađenja","Nom.","","kW","12.1 (1)"]
["Kapacitet grejanja","Nom.","","kW","13.5 (2)"]
["Hlađenje prostora","Kapacitet","Pdesign","kW","12.1"]
["","SEER","","","5.03"]
["","Godišnja potrošnja električne energije","","kWh/god.","1444"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","6"]
["","SCOP/A","","","3.58"]
["","Godišnja potrošnja električne energije","","kWh/god.","2346"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]