{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Kapacitet hlađenja","Ukupan kapacitet","","Nom.","kW","12.10","19.00","22.00"]
["Kapacitet grejanja","Ukupan kapacitet","","Nom.","kW","13.50","22.4","24.0"]
["Kućište","Boja","","","","Neofarbano","Neofarbano","Neofarbano"]
["","Materijal","","","","Galvanizovani čelik","Galvanizovana čelična ploča","Galvanizovana čelična ploča"]
["Dimenzije","Uređaj","","Visina","mm","300","470","470"]
["","","","Širina","mm","1,400","1,490","1,490"]
["","","","Dubina","mm","700","1,100","1,100"]
["Težina","Uređaj","","","kg","45","104","115"]
["Potrebna praznina plafona >","mm","","","","350"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","39.0","64.0","69.0"]
["","","","Srednji","m³/min","","50","56"]
["","","","Nizak","m³/min","28.0","36.0","43.0"]
["","","Grejanje","Visok","m³/min","39.0","64.0","69.0"]
["","","","Srednji","m³/min","","50.0","56.0"]
["","","","Nizak","m³/min","28.0","36.0","43.0"]
["","Spoljni statički pritisak","","Visok","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Nivo zvučne snage","Hlađenje","","","dBA","66","69.0","71.0"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Nizak","dBA","33","36.0","37.0"]
["","Grejanje","","Visok","dBA","40","43.0","44.0"]
["","","","Srednji","dBA","","39.0","40.0"]
["","","","Nizak","dBA","33","36.0","37.0"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","9.52","9.52"]
["","Gas","","SP","mm","15.90","19.1","22.2"]
["","Ispusni otvor","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Ispusna visina","mm","","","","625"]
["Ukrasni panel","Model","","","","BYBS125DJW1"]
["","Boja","","","","Bela (10Y9/0,5)"]
["","Dimenzije","","Visina","mm","55"]
["","","","širina","mm","1,500"]
["","","","Dubina","mm","500"]
["","Težina","","","kg","6.5"]
["Control systems","Infracrveni daljinski upravljač","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardni pribor","Navoji","","","","16","2","2"]
["","Podloška","","","","8","12","12"]
["","Traka za crevo","","","","1"]
["","Ispusno crevo","","","","1"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","1","1","1"]
["","Priručnik za montažu i upotrebu","","","","1","1","1"]
["","Kabl za zajedničko napajanje električnom energijom","","","","2"]
["","Materijal za fiksiranje (cev za odvod)","","","","1"]
["","Zaptivno sredstvo","","","","2"]
["","Termoizolaciona cev (tečnost)","","","","1"]
["","Termoizolaciona cev (gas)","","","","1"]
["Power supply","Ime","","","","","VE","VE"]
["","Faza","","","","1~","1~","1~"]
["","Frekvencija","","","Hz","50/60","50/60","50/60"]
["","Napon","","","V","220-240/220","220-240/220","220-240/220"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Standardni pribor","Priručnik za upotrebu","","","","","1","1"]
["","Priručnik za instalaciju","","","","","1","1"]
["","Spojna cev za gasovitu fazu","","","","","1","1"]
["","Materijal za spajanje žice","","","","","1","1"]
["","Opružna podloška","","","","","2","2"]
["","Zavrtanj+navrtka","","","","","45","45"]
["","Zavrtanj sa šestougaonom glavom sa podloškom","","","","","49","49"]
["","Zavrtanj sa šestougaonom glavom","","","","","2","2"]
["","Ravna podloška","","","","","8","8"]