{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RR-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9/RR125B8W1B"]
["Kapacitet hlađenja","Nom.","","kW","12.5 (1)"]
["Piping connections","Tečnost","SP","mm","9.52"]
["","Gas","SP","mm","15.9"]
["","Ispusni otvor","OD","mm","26"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","2,395"]
["","EER","","","2.61"]
["","Direktiva o energetskom označavanju","Hlađenje","","D"]
["Beleške","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]