{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RR-BW1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RR125B8W1B","FDQ125C5VEB / RR125B8W1B"]
["Kapacitet hlađenja","Nom.","","kW","12.2 (3)","12.2 (3)"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","2,260","2,260"]
["","EER","","","2.70","2.70"]
["","Direktiva o energetskom označavanju","Hlađenje","","D","D"]
["Beleške","","","","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)"]
["","","","","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)"]
["","","","","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19,0°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5 m (po horizontali); razlika nivoa: 0m","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19,0°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5 m (po horizontali); razlika nivoa: 0m"]
["","","","","(4) - U skladu sa EN/IEC 61000-3-11, poželjno je kontaktirati distributera da bi se osiguralo da je oprema priključena isključivo na napajanje sa Zsys vrednošću manjom ili jednakom sa Zsys (impedanca sistema) ≤ Zmax","(4) - U skladu sa EN/IEC 61000-3-11, poželjno je kontaktirati distributera da bi se osiguralo da je oprema priključena isključivo na napajanje sa Zsys vrednošću manjom ili jednakom sa Zsys (impedanca sistema) ≤ Zmax"]
["","","","","(5) - Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A.","(5) - Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A."]
["","","","","(6) - Impedanca sistema","(6) - Impedanca sistema"]
["","","","","(7) - Oprema u skladu sa standardom EN/IEC 61000-3-12: Evropski/internacionalni tehnički standard koji određuje granice za strujne harmonike koje proizvode jedinice priključene na nisko-naponsku javnu mrežu sa ulaznom strujom > 16A i ≤ 75A po fazi","(7) - Oprema u skladu sa standardom EN/IEC 61000-3-12: Evropski/internacionalni tehnički standard koji određuje granice za strujne harmonike koje proizvode jedinice priključene na nisko-naponsku javnu mrežu sa ulaznom strujom > 16A i ≤ 75A po fazi"]
["","","","","(8) - Struja kratkog spoja","(8) - Struja kratkog spoja"]
["","","","","(9) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(9) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]