{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L8Y1B","FDQ125C5VEB / RZQSG125L8Y1B"]
["Kapacitet hlađenja","Nom.","","kW","12.0","12.0"]
["Hlađenje prostora","SEER","","","5.2","5.2"]
["","Godišnja potrošnja električne energije","","kWh/god.","808","808"]
["","Kapacitet","Pdesign","kW","12","12"]
["","Klasa energetske efikasnosti","","","A","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","7.6","7.6"]
["","SCOP/A","","","3.9","3.9"]
["","Klasa energetske efikasnosti","","","A","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","2,729","2,729"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,870","1,870"]
["","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","B","B"]
["Kapacitet grejanja","Nom.","","kW","13.5","13.5"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]