{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Hlađenje prostora","SEER","","","4.35","4.35","4.35 (6)"]
["","Godišnja potrošnja električne energije","","kWh/god.","965.517","965.517"]
["","Kapacitet","Pdesign","kW","12.00","12.00"]
["","Klasa energetske efikasnosti","","","C","C"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Klasa energetske efikasnosti","","","A","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","2,791","2,791"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,600","1,870","1,870"]
["","EER","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A"]
["","","Grejanje","","B","B","B"]
["Kapacitet grejanja","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)"]
["","","","","","","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m"]
["","","","","","","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5 m; visinska razlika: 0m"]
["","","","","","","(5) - Godišnja potročnja energije je u skladu sa direktivom o energetskom označavanju 2002/31/EC"]
["","","","","","","(6) - SEER i SCOP su u skladu sa EN 14825"]
["","","","","","","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]