{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","","FDXM25F2V1B","FDXM35F2V1B","FDXM50F2V1B","FDXM60F2V1B"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Nom.","m³/min","8.0","8.0","11.0","14.8"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","33","33","36","35"]
["Ventilator","Brzina protoka vazduha","Grejanje","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["Nivo zvučnog pritiska","Grejanje","","Nom.","dBA","33","33","36","36"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Grejanje","","Nom.","kW","0.036","0.036","0.060","0.060"]
["Dimenzije","Uređaj","","Visina","mm","200","200","200","200"]
["","","","Širina","mm","750","750","1150","1150"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","620","620","620","620"]
["Težina","Uređaj","","","kg","21","21","30","30"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","8.7","8.7","12.0","16.0"]
["","","","Nizak","m³/min","7.3","7.3","10.0","13.5"]
["","","Grejanje","Visok","m³/min","8.7","8.7","16.0","16.0"]
["","","","Nizak","m³/min","7.3","7.3","13.5","13.5"]
["","Spoljni statički pritisak","","Nom.","Pa","30","30","40","40"]
["Nivo zvučne snage","Hlađenje","","","dBA","53","53","55","56"]
["","Grejanje","","","dBA","53","53","55","56"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","35","35","38","38"]
["","","","Nizak","dBA","27","27","30","30"]
["","Grejanje","","Visok","dBA","35","35","38","38"]
["","","","Nizak","dBA","27","27","30","30"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.5","9.5","12.7","12.7"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["","Žičani daljinski upravljač","","","","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A"]
["Napajanje","Ime","","","","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","230","230","220-240","220-240"]