{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM40M3V1B","FDXM25F3V1B / FDXM35F3V1B / 2MXM40M3V1B"]
["Kapacitet hlađenja","Nom.","","kW","4.0","4.0"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","563","555"]
["","EER","","","3.55","3.60"]
["","COP","","","4.13","4.17"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Kapacitet grejanja","Nom.","","kW","4.20","4.20"]
["Beleške","","","","(1) - Nominalni kapaciteti hlađenja se zasnivaju na: unutrašnjoj temperaturi: 27°CDB, 19°CWB, spoljašnjoj temperaturi: 35°CDB, odgovarajućoj dužini cevi rashladnog fluida: 5 m, visinskoj razlici: 0 m. Podaci za seriju standardne efikasnosti","(1) - Nominalni kapaciteti hlađenja se zasnivaju na: unutrašnjoj temperaturi: 27°CDB, 19°CWB, spoljašnjoj temperaturi: 35°CDB, odgovarajućoj dužini cevi rashladnog fluida: 5 m, visinskoj razlici: 0 m. Podaci za seriju standardne efikasnosti"]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]