{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / FDXM50F3V1B / RZAG71M7V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG71M7V1B","FDXM35F3V1B / FDXM35F3V1B / RZAG71M7V1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZAG100M7V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7V1B","FDXM50F3V1B / FDXM50F3V1B / RZAG100M7V1B"]
["Kapacitet hlađenja","Nom.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Space cooling","SEER","","","7.12","6.32","6.27","8.77","8.00","7.86","8.60"]
["","Godišnja potrošnja električne energije","","kWh/a","334","377","380","379","416","423","387"]
["","Kapacitet","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50"]
["","Klasa energetske efikasnosti","","","A++","A++","A++","A+++","A++","A++","A+++"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.70","4.70","4.70","7.80","7.80","7.80","7.80"]
["","SCOP/A","","","4.43","4.28","4.14","4.70","4.48","4.30","4.51"]
["","Klasa energetske efikasnosti","","","A+","A+","A+","A++","A+","A+","A+"]
["","Godišnja potrošnja električne energije","","kWh/a","1,485","1,537","1,589","2,324","2,438","2,540","2,421"]
["Kapacitet grejanja","Nom.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]