{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B","FDXM60F3V1B9 / RXM60A5V1B"]
["Kapacitet hlađenja","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.00","6"]
["","Maks.","","kW","5.30","6.5"]
["Kapacitet grejanja","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.80","7"]
["","Maks.","","kW","6.00","7.1"]
["Nominalna efikasnost","EER","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Godišnja potrošnja električne energije","","kWh","817","1024"]
["","Direktiva o energetskom označavanju","Hlađenje","","B","C"]
["","","Grejanje","","D","C"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+","A"]
["","Kapacitet","Pdesign","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Godišnja potrošnja električne energije","","kWh/a","303","378"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A","A"]
["","Kapacitet","Pdesign","kW","4.00","4.6"]
["","SCOP/A","","","3.93","3.8"]
["","Pdh Kapacitet grejanja na -10°C","","kW","3.54","3.94"]
["","Godišnja potrošnja električne energije","","kWh/a","1424","1693"]
["Beleške","","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]