{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXM25A5V1B9","FDXM35F3V1B9 / RXM35A5V1B9","FDXM50F3V1B9 / RXM50A5V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","2.4","3.4","5"]
["","Maks.","","kW","3","3.8","5.3"]
["Kapacitet grejanja","Min.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","3.2","4","5.8"]
["","Maks.","","kW","4.5","5","6"]
["Nominalna efikasnost","EER","","","3.77","2.98","3.06"]
["","COP","","","4","3.48","3.1"]
["","Godišnja potrošnja električne energije","","kWh","318","570","817"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","C","B"]
["","","Grejanje","","A","B","D"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+","A","A+"]
["","Kapacitet","Pdesign","kW","2.4","3.4","5"]
["","SEER","","","5.79","5.35","5.77"]
["","Godišnja potrošnja električne energije","","kWh/a","145","222","303"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A+","A","A"]
["","Kapacitet","Pdesign","kW","2.6","2.9","4"]
["","SCOP/A","","","4.29","3.95","3.93"]
["","Pdh Kapacitet grejanja na -10°C","","kW","2.15","2.32","3.54"]
["","Godišnja potrošnja električne energije","","kWh/a","848","1028","1424"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]