{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Grejanje","","Nom.","kW","0.036","0.036","0.060","0.060"]
["Dimenzije","Uređaj","","Visina","mm","200","200","200","200"]
["","","","Širina","mm","750","750","1150","1150"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","620","620","620","620"]
["Težina","Uređaj","","","kg","21","21","28","28"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","8.7","8.7","15.8","16.0"]
["","","","Srednji","m³/min","8.0","8.0","14.6","14.8"]
["","","","Nizak","m³/min","7.3","7.3","13.3","13.5"]
["","","Grejanje","Visok","m³/min","8.7","8.7","15.8","16.0"]
["","","","Srednji","m³/min","8.0","8.0","14.6","14.8"]
["","","","Nizak","m³/min","7.3","7.3","13.3","13.5"]
["","Spoljni statički pritisak","","Nom.","Pa","30","30","40","40"]
["Nivo zvučne snage","Hlađenje","","","dBA","53.0","53.0","55.0","56.0"]
["","Grejanje","","","dBA","53.0","53.0","55.0","56.0"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","35.0","35.0","38.0","38.0"]
["","","","Srednji","dBA","33.0","33.0","35.0","35.0"]
["","","","Nizak","dBA","27.0","27.0","30.0","30.0"]
["","Grejanje","","Visok","dBA","35.0","35.0","38.0","38.0"]
["","","","Srednji","dBA","33.0","33.0","35.0","35.0"]
["","","","Nizak","dBA","27.0","27.0","30.0","30.0"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.50","9.50","12.70","12.70"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Clamps","","","","6","6","6","6"]
["","Drain hose","","","","1","1","1","1"]
["","Filter za vazduh","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Sealing material","","","","2","2","2","2"]
["","Sealing pad","","","","1","1","1","1"]
["","Washer fixing plate","","","","4","4","4","4"]
["Opseg energetske efikasnosti","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]