{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","35.0","35.0","","38.0"]
["","","","Srednji","dBA","33.0","33.0","","35.0"]
["","","","Nizak","dBA","27.0","27.0","","30.0"]
["","Hlađenje","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Nizak","dBA","27.0","27.0","","30.0"]
["","","","Visok","dBA","35.0","35.0","","38.0"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1","","1"]
["","Priručnik za upotrebu","","","","1","1","","1"]
["","Izolacija za fiting","","","","1","1","","1"]
["","Zaptivna pločica","","","","1","1","","1"]
["","Stezni metal","","","","1","1","","1"]
["","Ispusno crevo","","","","1","1","","1"]
["","Podloška vešaljke","","","","8","8","","8"]
["","Zaptivno sredstvo","","","","2","2","","2"]
["","Obujmice","","","","6","6","","6"]
["","Podloška pričvrsne ploče","","","","4","4","","4"]
["","Zavrtnji cevnih prirubnica","","","","1","1","","1"]
["","Filter za vazduh","","","","1","1","","1"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","","6.35"]
["","Gas","","SP","mm","9.50","9.50","","12.70"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.036","0.036","","0.060"]
["","Grejanje","","Nom.","kW","0.036","0.036","","0.060"]
["Nivo zvučne snage","Hlađenje","","","dBA","53.0","53.0","","56.0"]
["","Grejanje","","","dBA","53.0","53.0","","56.0"]
["Dimenzije","Uređaj","","Širina","mm","750","750","","1,150"]
["","","","Dubina","mm","620","620","","620"]
["","","","Visina","mm","200","200","","200"]
["Težina","Uređaj","","","kg","21","21","","28"]
["Ventilator","Spoljni statički pritisak","","Nom.","Pa","30","30","","40"]
["","Brzina protoka vazduha","Grejanje","Visok","m³/min","8.7","8.7","","16.0"]
["","","","Srednji","m³/min","8.0","8.0","","14.8"]
["","","","Nizak","m³/min","7.3","7.3","","13.5"]
["","","Hlađenje","Nizak","m³/min","7.3","7.3","","13.5"]
["","","","Srednji","m³/min","8.0","8.0","","14.8"]
["","","","Visok","m³/min","8.7","8.7","","16.0"]
["Power supply","Faza","","","","1~","1~","","1~"]
["","Frekvencija","","","Hz","50","50","","50"]
["","Napon","","","V","220-240","220-240","","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","","0.060"]
["","Grejanje","","Nom.","kW","","","0.060"]
["Dimenzije","Uređaj","","Visina","mm","","","200"]
["","","","Širina","mm","","","1150"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","","620"]
["Težina","Uređaj","","","kg","","","28"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","","15.8"]
["","","","Srednji","m³/min","","","14.6"]
["","","","Nizak","m³/min","","","13.3"]
["","","Grejanje","Visok","m³/min","","","15.8"]
["","","","Srednji","m³/min","","","14.6"]
["","","","Nizak","m³/min","","","13.3"]
["","Spoljni statički pritisak","","Nom.","Pa","","","40"]
["Nivo zvučne snage","Hlađenje","","","dBA","","","55.0"]
["","Grejanje","","","dBA","","","55.0"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","","38.0"]
["","","","Srednji","dBA","","","35.0"]
["","","","Nizak","dBA","","","30.0"]
["","Grejanje","","Visok","dBA","","","38.0"]
["","","","Srednji","dBA","","","35.0"]
["","","","Nizak","dBA","","","30.0"]
["Povezivanje cevi","Tečnost","","SP","mm","","","6.35"]
["","Gas","","SP","mm","","","12.70"]
["","Ispusni otvor","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardni pribor","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Napajanje","Faza","","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","","50"]
["","Napon","","","V","","","220-240"]