{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXL-K"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXL25K3V1B","FDXS35F2VEB / RXL35K2V1B","FDXS50F2VEB / RXL50K2V1B"]
["Kapacitet hlađenja","Min.","","kW","","1.4","1.7"]
["","Maks.","","kW","","3.8","5.3"]
["","Nom.","","kW","2.40","3.4","5.0"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","345","530","825"]
["","EER","","","3.48","3.21","3.03"]
["","COP","","","3.52","3.47","3.10"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","B"]
["","","Grejanje","","B","B","D"]
["Kapacitet grejanja","Nom.","","kW","3.20","4.10","5.80"]
["","Min.","","kW","","1.40","1.70"]
["","Maks.","","kW","","5.00","6.00"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]