{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Kapacitet hlađenja","Min.","","kW","1.7"]
["","Maks.","","kW","6.5"]
["","Nom.","","kW","6.0 (2)"]
["Cevne spojnice","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","12.7"]
["","Ispusni otvor","OD","mm","VP20 (Spoljni preč.26, Unutrašnji preč. 20)"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,030"]
["","EER","","","2.91 (1)"]
["","COP","","","3.21 (1)"]
["","Direktiva o energetskom označavanju","Hlađenje","","C"]
["","","Grejanje","","C"]
["Kapacitet grejanja","Nom.","","kW","7.0 (3)"]
["","Min.","","kW","1.7"]
["","Maks.","","kW","8.0"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","(4) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]