{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB","FDXS35F2VEB","FDXS60F2VEB"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","35","35","38"]
["","","Srednji","dBA","33","33","36"]
["","","Nizak","dBA","27","27","30"]
["","Hlađenje","Srednji","dBA","33","33","35"]
["","","Nizak","dBA","27","27","30"]
["","","Visok","dBA","35","35","38"]
["Standardni pribor","Priručnik za instalaciju","","","1","1","1"]
["","Priručnik za upotrebu","","","1","1","1"]
["","Izolacija za fiting","","","1","1","1"]
["","Zaptivna pločica","","","1","1","1"]
["","Stezni metal","","","1","1","1"]
["","Ispusno crevo","","","1","1","1"]
["","Podloška vešaljke","","","8","8","8"]
["","Zaptivno sredstvo","","","2","2","2"]
["","Obujmice","","","6","6","6"]
["","Podloška pričvrsne ploče","","","4","4","4"]
["","Zavrtnji cevnih prirubnica","","","1","1","1"]
["","Filter za vazduh","","","1","1","1"]
["Povezivanje cevi","Tečnost","SP","mm","6.35","6.35","6.35"]
["","Gas","SP","mm","9.50","9.50","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ulazna snaga","Hlađenje","Nom.","kW","0.036","0.036","0.060"]
["","Grejanje","Nom.","kW","0.036","0.036","0.060"]
["Sound power level","Hlađenje","","dBA","53","53","56"]
["","Grejanje","","dBA","53","53","56"]
["Dimenzije","Uređaj","Širina","mm","750","750","1,150"]
["","","Dubina","mm","620","620","620"]
["","","Visina","mm","200","200","200"]
["Težina","Uređaj","","kg","21.0","21.0","30.0"]
["Ventilator","Spoljni statički pritisak","Nom.","Pa","30","30","40"]
["Power supply","Faza","","","1~","1~","1~"]
["","Frekvencija","","Hz","50/60","50/60","50/60"]
["","Ime","","","VE","VE","VE"]
["","Napon","","V","220-240","220-240","220-240"]
["Beleške","","","","(1) - Radni nivo zvuka se zasniva na zadnjoj strani usisnog otvora i spoljni statički pritisak (ESP) 40Pa. Radni nivo zvuka za donju stranu usis. otvora: (radni nivo zvuka na zadnje strane usis. otvora) +5 dB. Međutim, kod instal. kod kojih postoji nizak spoljni statički pritisak (ESP), može doći do povećanja nivoa zvuka i iznad 5 dB.","(1) - Radni nivo zvuka se zasniva na zadnjoj strani usisnog otvora i spoljni statički pritisak (ESP) 40Pa. Radni nivo zvuka za donju stranu usis. otvora: (radni nivo zvuka na zadnje strane usis. otvora) +5 dB. Međutim, kod instal. kod kojih postoji nizak spoljni statički pritisak (ESP), može doći do povećanja nivoa zvuka i iznad 5 dB.","(1) - Radni nivo zvuka se zasniva na zadnjoj strani usisnog otvora i spoljni statički pritisak (ESP) 40Pa. Radni nivo zvuka za donju stranu usis. otvora: (radni nivo zvuka na zadnje strane usis. otvora) +5 dB. Međutim, kod instal. kod kojih postoji nizak spoljni statički pritisak (ESP), može doći do povećanja nivoa zvuka i iznad 5 dB."]
["","","","","(2) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu.","(2) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu.","(2) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu."]