{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / FDXS50F2VEB9 / FDXS50F2VEB9 / RZQSG125L8Y1B"]
["Hlađenje prostora","SEER","","","4.8"]
["","Godišnja potrošnja električne energije","","kWh/god.","875"]
["","Kapacitet","Pdesign","kW","12"]
["","Klasa energetske efikasnosti","","","B"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","7.6"]
["","SCOP/A","","","3.8"]
["","Klasa energetske efikasnosti","","","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","2,800"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]