{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","38"]
["","","Srednji","dBA","36"]
["","","Nizak","dBA","30"]
["","Hlađenje","Medium","dBA","36"]
["","","Nizak","dBA","30"]
["","","Visok","dBA","38"]
["Standardni pribor","Priručnik za instalaciju","","","1"]
["","Priručnik za upotrebu","","","1"]
["","Izolacija za fiting","","","1"]
["","Zaptivna pločica","","","1"]
["","Stezni metal","","","1"]
["","Ispusno crevo","","","1"]
["","Podloška vešaljke","","","8"]
["","Zaptivno sredstvo","","","2"]
["","Obujmice","","","6"]
["","Podloška pričvrsne ploče","","","4"]
["","Zavrtnji cevnih prirubnica","","","1"]
["","Filter za vazduh","","","1"]
["Piping connections","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","12.7"]
["","Ispusni otvor","","","VP20 (I.D. 20/O.D. 26)"]
["Apsorbovana snaga","Hlađenje","Nom.","kW","0.060"]
["","Grejanje","Nom.","kW","0.060"]
["Nivo zvučne snage","Hlađenje","","dBA","55"]
["","Grejanje","","dBA","55"]
["Dimenzije","Uređaj","Širina","mm","1,150"]
["","","Dubina","mm","620"]
["","","Visina","mm","200"]
["Težina","Uređaj","","kg","30.0"]
["Ventilator","Spoljni statički pritisak","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frekvencija","","Hz","50/60"]
["","Ime","","","VE"]
["","Napon","","V","220-240"]
["Beleške","","","","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu."]