{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXS50L2V1B","FFA60A2VEB / RXS60L2V1B"]
["Kapacitet hlađenja","Nom.","","kW","5.00","5.70"]
["Hlađenje prostora","SEER","","","5.93","5.71"]
["","Godišnja potrošnja električne energije","","kWh/a","295","349"]
["","Kapacitet","Pdesign","kW","5.00","5.70"]
["","Klasa energetske efikasnosti","","","A+","A+"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","3.84","3.96"]
["","SCOP/A","","","3.90","4.04"]
["","Klasa energetske efikasnosti","","","A","A+"]
["","Godišnja potrošnja električne energije","","kWh/a","1,378","1,373"]
["Piping connections","Tečnost","SP","mm","6.35","6.35"]
["","Gas","SP","mm","12.70","12.70"]
["","Ispusni otvor","OD","mm","VP20 (Spoljni preč.26, Unutrašnji preč. 20)","VP20 (Spoljni preč.26, Unutrašnji preč. 20)"]
["Nominalna efikasnost","EER","","","3.21","3.02"]
["","Godišnja potrošnja električne energije","","kWh","780","945"]
["","COP","","","3.49","3.41"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","B"]
["","","Grejanje","","B","B"]
["Kapacitet grejanja","Nom.","","kW","5.80","7.00"]
["Beleške","","","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]