{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Kućište","Materijal","","","","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča"]
["Dimenzije","Uređaj","","Visina","mm","260","260","260","260"]
["","","","Širina","mm","575","575","575","575"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","575","575","575","575"]
["Težina","Uređaj","","","kg","16.0","16.0","17.5","17.5"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","9.0","10.0","12.0","14.5"]
["","","","Srednji","m³/min","8.0","8.5","10.0","12.5"]
["","","","Nizak","m³/min","6.5","6.5","7.5","9.5"]
["","","Grejanje","Visok","m³/min","9.0","10.0","12.0","14.5"]
["","","","Srednji","m³/min","8.0","8.5","10.0","12.5"]
["","","","Nizak","m³/min","6.5","6.5","7.5","9.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","48","51","56","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","31.0","34.0","39.0","43.0"]
["","","","Srednji","dBA","28.5","30.5","34.0","40.0"]
["","","","Nizak","dBA","25.0","25.0","27.0","32.0"]
["","Grejanje","","Visok","dBA","31.0","34.0","39.0","43.0"]
["","","","Srednji","dBA","28.5","30.5","34.0","40.0"]
["","","","Nizak","dBA","25.0","25.0","27.0","32.0"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.52","9.52","12.70","12.70"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Ukrasna maska","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Boja","","","","Bela (N9.5)","Bela (N9.5)","Bela (N9.5)","Bela (N9.5)"]
["","Dimenzije","","Visina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Dubina","mm","620","620","620","620"]
["","Težina","","","kg","2.8","2.8","2.8","2.8"]
["Ukrasni panel 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Boja","","","","Srebrna","Srebrna","Srebrna","Srebrna"]
["","Dimenzije","","Visina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Dubina","mm","620","620","620","620"]
["","Težina","","","kg","2.8","2.8","2.8","2.8"]
["Ukrasni panel 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Boja","","","","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)"]
["","Dimenzije","","Visina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Dubina","mm","700","700","700","700"]
["","Težina","","","kg","2.7","2.7","2.7","2.7"]
["Ukrasni panel 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Boja","","","","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)"]
["","Dimenzije","","Visina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Dubina","mm","700","700","700","700"]
["","Težina","","","kg","2.7","2.7","2.7","2.7"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","BRC7EB530 (standardna maska), BRC7F530W (bela maska), BRC7F530S (siva maska)","BRC7EB530 (standardna maska), BRC7F530W (bela maska), BRC7F530S (siva maska)","BRC7EB530 (standardna maska), BRC7F530W (bela maska), BRC7F530S (siva maska)","BRC7EB530 (standardna maska), BRC7F530W (bela maska), BRC7F530S (siva maska)"]
["","Žičani daljinski upravljač","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardni pribor","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]