{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Kapacitet hlađenja","Nom.","","kW","","","","","","","","6.80 (1)"]
["Hlađenje prostora","SEER","","","","","","","","5.10","5.10","6.86","5.10","5.10","5.10","5.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","467","467","347","467","652","652","652"]
["","Kapacitet","Pdesign","kW","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Klasa energetske efikasnosti","","","","","","","","A","A","A++","A","A","A","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","","","","","","6.00","6.00","7.60","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","3.80","4.32","3.80","3.80","3.80","3.80"]
["","Klasa energetske efikasnosti","","","","","","","","A","A","A+","A","A","A","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","2,211","2,211","2,463","2,211","4,164","4,164","4,164"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","","","","","","","","890"]
["","EER","","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","","4.13 (3)"]
["","Direktiva o energetskom označavanju","Hlađenje","","","","","","","","","A"]
["","","Grejanje","","","","","","","","","A"]
["Kapacitet grejanja","Nom.","","kW","","","","","","","","7.50 (2)"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Beleške","","","","","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 7,5m; visinska razlika: 0m"]
["","","","","","","","","","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","","(3) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","","","","","","","","","","","A"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","","","","","824"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","","","","","","","","","","","A"]
["","Kapacitet","Pdesign","kW","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Pdh Kapacitet grejanja na -10°C","","kW","","","","","","","","","","","","","11"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","","","","","4683"]