{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Srednji","dBA","31","32","33","34"]
["","Hlađenje","Medium","dBA","34","35","35","36"]
["","","Nizak","dBA","31","32","33","34"]
["","","Visok","dBA","36","37","37","38"]
["Standardni pribor","Termoizolaciona cev","","","2","2","2","2"]
["","Materijal za spajanje žice","","","7","7","7","7"]
["","Traka za crevo","","","1","1","1","1"]
["","Ispusno crevo","","","1","1","1","1"]
["","Podloška","","","8","8","8","8"]
["","Zaptivna pločica (velika)","","","1","1","1","1"]
["","Zaptivna pločica (mala)","","","1","1","1","1"]
["","Smolasta patrona","","","1","1","1","1"]
["","Navoji","","","2","2","2","2"]
["","Oprema za ožičavanje","","","2","2","2","2"]
["Control systems","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infracrveni daljinski upravljač","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Povezivanje cevi","Tečnost","SP","mm","6.35","6.35","6.35","9.52"]
["","Gas","SP","mm","9.50","12.7","12.7","15.9"]
["","Ispusni otvor","","","VP20","VP20","VP20","VP20"]
["Nivo zvučne snage","Hlađenje","","dBA","53","54","54","55"]
["Dimenzije","Uređaj","Širina","mm","960","960","1,270","1,270"]
["","","Dubina","mm","690","690","690","690"]
["","","Visina","mm","235","235","235","235"]
["Kućište","Materijal","","","Smola, metalna ploča","Smola, metalna ploča","Smola, metalna ploča","Smola, metalna ploča"]
["","Boja","","","Bela","Bela","Bela","Bela"]
["Težina","Uređaj","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Faza","","","1~","1~","1~","1~"]
["","Frekvencija","","Hz","50","50","50","50"]
["","Napon","","V","220-240","220-240","220-240","220-240"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]