{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RR-BV3"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RR71B8V3B","FHQ100CAVEB / RR100B8V3B"]
["Kapacitet hlađenja","Nom.","","kW","7.1 (3)","9.8 (3)"]
["Piping connections","Tečnost","SP","mm","9.52","9.52"]
["","Gas","OD","mm","15.9","15.9"]
["","Ispusni otvor","OD","mm","26","26"]
["Nominalna efikasnost","Annual energy consumption","","kWh","1,350","1,875"]
["","EER","","","2.63","2.61"]
["","Direktiva o energetskom označavanju","Hlađenje","","D","D"]
["Beleške","","","","(1) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)","(1) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)"]
["","","","","(2) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)","(2) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)"]
["","","","","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m","(3) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 7,5m; visinska razlika: 0m"]
["","","","","(4) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(4) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]