{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Kapacitet hlađenja","Min.","","kW","1.2"]
["","Maks.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Piping connections","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","9.5"]
["","Ispusni otvor","OD","mm","18.0"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Direktiva o energetskom označavanju","Hlađenje","","B"]
["","","Grejanje","","B"]
["Kapacitet grejanja","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Maks.","","kW","5.0"]
["Beleške","","","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - 220V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240V"]
["","","","","(5) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","(6) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]