{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","46"]
["","","Nečujan rad","dBA","30"]
["","","Nizak","dBA","33"]
["","Hlađenje","Nečujan rad","dBA","29"]
["","","Nizak","dBA","32"]
["","","Visok","dBA","38"]
["","","Nom.","dBA","36"]
["","Hlađenje","Nom.","dBA","35"]
["Standardni pribor","Priručnik za instalaciju","","","1"]
["","Priručnik za upotrebu","","","1"]
["","Infracrveni daljinski upravljač","","","1"]
["","AAA suve baterije","","","2"]
["","Držač daljinskog upravljača","","","1"]
["","Noseća ploča","","","1"]
["","Termoizolovana cev (cev za rashladni fluid)","","","8"]
["","Filter za vazduh","","","1"]
["","Fotokatalitički deodorišući filter","","","1"]
["","Bočni poklopac","","","2"]
["","Traka za obavijanje","","","4"]
["Kontrolni sistemi","Infrared remote control","","","ARC433B67"]
["Piping connections","Tečnost","SP","mm","6.35"]
["","Gas","SP","mm","9.5"]
["","Ispusni otvor","","","18"]
["Nivo zvučne snage","Hlađenje","","dBA","53"]
["","Grejanje","","dBA","59"]
["Dimenzije","Uređaj","Širina","mm","1,050"]
["","","Dubina","mm","200"]
["","","Visina","mm","490"]
["Kućište","Colour","","","Badem bela"]
["Težina","Uređaj","","kg","16"]
["Power supply","Phase","","","1~"]
["","Frekvencija","","Hz","50"]
["","Ime","","","VM"]
["","Napon","","V","220-240"]
["Beleške","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu."]