{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FNA35A2VEB9 / FNA35A2VEB9 / RZQG71L9V1B","FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / RZQG100L9V1B","FNA50A2VEB9 / FNA50A2VEB9 / RZQG100L9V1B","FNA60A2VEB9 / FNA60A2VEB9 / RZQG125L9V1B","FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / FNA35A2VEB9 / RZQG125L9V1B","FNA50A2VEB9 / FNA50A2VEB9 / FNA50A2VEB9 / RZQG125L9V1B"]
["Kapacitet hlađenja","Nom.","","kW","6.80","9.50","9.50","12.00","12.00","12.00"]
["Hlađenje prostora","SEER","","","4.80","5.10","5.10","5.10","5.10","5.10"]
["","Godišnja potrošnja električne energije","","kWh/a","496","652","652","824","824","824"]
["","Kapacitet","Pdesign","kW","6.80","9.50","9.50","12.00","12.00","12.00"]
["","Klasa energetske efikasnosti","","","B","A","A","A","A","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","6.00","10.74","11.30","12.71","11.30","12.71"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Klasa energetske efikasnosti","","","A","A","A","A","A","A"]
["","Godišnja potrošnja električne energije","","kWh/a","2,211","3,957","4,164","4,683","4,164","4,683"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","1,111","1,405","1,257","1,875","1,967","1,724"]
["","EER","","","3.06","3.38","3.78","3.20","3.05","3.48"]
["","COP","","","2.94","2.93","3.65","3.21","3.03","3.74"]
["","Direktiva o energetskom označavanju","Hlađenje","","B","A","A","B","B","A"]
["","","Grejanje","","D","D","A","C","D","A"]
["Kapacitet grejanja","Nom.","","kW","7.50","10.80","10.80","13.50","13.50","13.50"]
["Beleške","","","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]