{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","33.0","33.0","36.0","36.0"]
["","","","Nom.","dBA","31.0","31.0","33.0","33.0"]
["","","","Nizak","dBA","28.0","28.0","30.0","30.0"]
["","Hlađenje","","Medium","dBA","31.0","31.0","33.0","33.0"]
["","","","Nizak","dBA","28.0","28.0","30.0","30.0"]
["","","","Visok","dBA","33.0","33.0","36.0","36.0"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infracrveni daljinski upravljač","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.52","9.52","12.7","12.7"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Nivo zvučne snage","Hlađenje","","","dBA","53.0","53.0","56.0","56.0"]
["Dimenzije","Uređaj","","Širina","mm","790","790","1,190","1,190"]
["","","","Dubina","mm","200","200","200","200"]
["","","","Visina","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Kućište","Materijal","","","","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča"]
["","Boja","","","","Neofarbano","Neofarbano","Neofarbano","Neofarbano"]
["Težina","Uređaj","","","kg","23.0","23.0","30.0","30.0"]
["Ventilator","Spoljni statički pritisak","","Visok","Pa","48","48","49","49"]
["","","","Nom.","Pa","30","30","40","40"]
["","Brzina protoka vazduha","Grejanje","Visok","m³/min","8.7","8.7","16.0","16.0"]
["","","","Nizak","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","Hlađenje","Nizak","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","","Visok","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Faza","","","","1~","1~","1~","1~"]
["","Ime","","","","VE","VE","VE","VE"]
["","Frekvencija","","","Hz","50/60","50/60","50/60","50/60"]
["","Napon","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Beleške","","","","","(1) - Uključujući montažne nosače","(1) - Uključujući montažne nosače","(1) - Uključujući montažne nosače","(1) - Uključujući montažne nosače"]
["","","","","","(2) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(2) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(2) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(2) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka."]