{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["","","Nizak","dBA","28","28","30","30"]
["","Hlađenje","Nizak","dBA","28","28","30","30"]
["","","Visok","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["Rashladno sredstvo","GWP (potencijal globalnog otopljavanja)","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Kapacitet hlađenja","Ukupan kapacitet","Nom.","kW","2.6","3.4","5.0","6.0"]
["Piping connections","Tečnost","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","SP","mm","9.52","9.52","12.7","12.7"]
["","Ispusni otvor","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Nivo zvučne snage","Hlađenje","","dBA","53","53","56","56"]
["Dimenzije","Uređaj","Širina","mm","790","790","1,190","1,190"]
["","","Dubina","mm","200","200","200","200"]
["","","Visina","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Kućište","Materijal","","","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča","Galvanizovana čelična ploča"]
["","Colour","","","Neofarbano","Neofarbano","Neofarbano","Neofarbano"]
["Težina","Uređaj","","kg","23","23","30","30"]
["Ventilator","Spoljni statički pritisak","Visok","Pa","48","48","49","49"]
["","","Nom.","Pa","30","30","40","40"]
["Kapacitet grejanja","Ukupan kapacitet","Nom.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frekvencija","","Hz","50/60","50/60","50/60","50/60"]
["","Napon","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Beleške","","","","(1) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(1) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(1) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka.","(1) - Nivo zvučne snage je apsolutna vrednost koja predstavlja \"snagu\" koju stvara izvor zvuka."]
["","","","","(2) - Uključujući montažne nosače","(2) - Uključujući montažne nosače","(2) - Uključujući montažne nosače","(2) - Uključujući montažne nosače"]