{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":9,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","39","40","","46"]
["","","","Srednji","dBA","32","33","","42"]
["","","","Nečujan rad","dBA","19","19","","24"]
["","","","Nizak","dBA","25","25","","33"]
["","Hlađenje","","Srednji","dBA","32","33","","39"]
["","","","Nečujan rad","dBA","19","19","","24"]
["","","","Nizak","dBA","25","25","","31"]
["","","","Visok","dBA","39","40","","46"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1","","1"]
["","Priručnik za upotrebu","","","","1","1","","1"]
["","Filter za vazduh","","","","2","2","","2"]
["","Infracrveni daljinski upravljač","","","","1","1","","1"]
["","Noseća ploča daljinskog upravljača","","","","1","1","","1"]
["","Vreća za zavrtnje","","","","1","1","","1"]
["","Poklopac zavrtnja","","","","1","1","","1"]
["","AAA suve baterije","","","","2","2","","2"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","1","1","","1"]
["Rashladno sredstvo","GWP","","","","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","","BRC073"]
["","Infracrveni daljinski upravljač","","","","ARC466A58","ARC466A58","","ARC466A58"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","","6.35"]
["","Gas","","SP","mm","9.50","9.50","","12.70"]
["","Ispusni otvor","","","","18","18","","18"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.020","0.022","","0.030"]
["","Grejanje","","Nom.","kW","0.020","0.020","","0.039"]
["Nivo zvučne snage","Hlađenje","","","dBA","57","57","","60"]
["Dimenzije","Uređaj","","širina","mm","798","798","","798"]
["","","","Dubina","mm","189","189","","189"]
["","","","Visina","mm","295","295","","295"]
["Casing","Boja","","","","Bela","Bela","","Bela"]
["Težina","Uređaj","","","kg","11.50","11.50","","11.50"]
["Fan","Brzina protoka vazduha","Grejanje","Visok","m³/min","10.9","11.1","","15.1"]
["","","","Srednji","m³/min","8.7","9.0","","11.1"]
["","","","Nizak","m³/min","6.4","6.4","","8.2"]
["","","","Nečujan rad","m³/min","4.5","4.5","","5.7"]
["","","Hlađenje","Nizak","m³/min","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","","10.4"]
["","","","Visok","m³/min","11.0","11.5","","13.5"]
["","","","Nečujan rad","m³/min","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Ime","","","","V1","V1","","V1"]
["","Frekvencija","","","Hz","50","50","","50"]
["","Napon","","","V","220-240","220-240","","220-240"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","","0.028"]
["","Grejanje","","Nom.","kW","","","0.036"]
["Kućište","Boja","","","","","","Bela"]
["Dimenzije","Uređaj","","Visina","mm","","","295"]
["","","","Širina","mm","","","798"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","","189"]
["Težina","Uređaj","","","kg","","","11.50"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","","13.1"]
["","","","Srednji","m³/min","","","9.8"]
["","","","Nizak","m³/min","","","7.2"]
["","","","Nečujan rad","m³/min","","","4.6"]
["","","Grejanje","Visok","m³/min","","","14.6"]
["","","","Srednji","m³/min","","","10.5"]
["","","","Nizak","m³/min","","","7.7"]
["","","","Nečujan rad","m³/min","","","5.2"]
["Nivo zvučne snage","Hlađenje","","","dBA","","","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","","45"]
["","","","Srednji","dBA","","","37"]
["","","","Nizak","dBA","","","29"]
["","","","Nečujan rad","dBA","","","21"]
["","Grejanje","","Visok","dBA","","","45"]
["","","","Srednji","dBA","","","37"]
["","","","Nizak","dBA","","","29"]
["","","","Nečujan rad","dBA","","","21"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","","","675.0"]
["Povezivanje cevi","Tečnost","","SP","mm","","","6.35"]
["","Gas","","SP","mm","","","12.70"]
["","Ispusni otvor","","","","","","18"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","","","ARC466A58"]
["","Žičani daljinski upravljač","","","","","","BRC073"]
["Standardni pribor","Installation manual","","","","","","1"]
["","Screw cover","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","General safety precautions","","","","","","1"]
["","Operation manual","","","","","","1"]
["","Filter za vazduh","","","","","","2"]
["","Infrared remote control","","","","","","1"]
["","Remote controller mounting plate","","","","","","1"]
["","Screw bag","","","","","","1"]
["Napajanje","Ime","","","","","","V1"]
["","Faza","","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","","50"]
["","Napon","","","V","","","220-240"]