{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BS / RXA-A8"]
[]
[]
[]
[]
["","","","","FTXA20B2V1BS / RXA20A5V1B8","FTXA25B2V1BS / RXA25A5V1B8","FTXA35B2V1BS / RXA35A5V1B8"]
["Kapacitet hlađenja","Min.","","kW","1.30","1.30","1.40"]
["","Nom.","","kW","2.00","2.50","3.40"]
["","Maks.","","kW","2.60","3.20","4.00"]
["Kapacitet grejanja","Min.","","kW","1.30","1.30","1.40"]
["","Nom.","","kW","2.50","2.80","4.00"]
["","Maks.","","kW","3.50","4.70","5.20"]
["Nominalna efikasnost","EER","","","4.70","4.46","4.37"]
["","COP","","","5.00","5.00","4.04"]
["","Godišnja potrošnja električne energije","","kWh","213","280","389"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A"]
["","","Grejanje","","A","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+++","A+++","A+++"]
["","Kapacitet","Pdesign","kW","2.00","2.50","3.40"]
["","SEER","","","8.75","8.74","8.73"]
["","Godišnja potrošnja električne energije","","kWh/god.","80","100","136"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A+++","A+++","A+++"]
["","Kapacitet","Pdesign","kW","2.40","2.45","2.50"]
["","SCOP/A","","","5.15","5.15","5.15"]
["","Pdh Kapacitet grejanja na -10°C","","kW","2.04","2.09","2.10"]
["","Godišnja potrošnja električne energije","","kWh/god.","652","666","680"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]