{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-B8"]
[]
[]
[]
[]
["","","","","FTXA42C2V1BW / RXA42B5V1B8","FTXA50C2V1BW / RXA50B5V1B8"]
["Kapacitet hlađenja","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","4.2","5"]
["","Maks.","","kW","5","5.3"]
["Kapacitet grejanja","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","5.4","5.8"]
["","Maks.","","kW","6","6.5"]
["Nominalna efikasnost","EER","","","3.99","3.68"]
["","COP","","","4.12","4"]
["","Godišnja potrošnja električne energije","","kWh","526","679"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A++","A++"]
["","Kapacitet","Pdesign","kW","4.2","5"]
["","SEER","","","7.5","7.33"]
["","Godišnja potrošnja električne energije","","kWh/god.","196","239"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","A++"]
["","Kapacitet","Pdesign","kW","3.8","4"]
["","SCOP/A","","","4.6","4.6"]
["","Pdh Kapacitet grejanja na -10°C","","kW","3.04","3.19"]
["","Godišnja potrošnja električne energije","","kWh/god.","1,156","1,218"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]