{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-C / RXC-C"]
[]
[]
[]
[]
["","","","","FTXC20CV1B / RXC20CV1B","FTXC25CV1B / RXC25CV1B","FTXC35CV1B / RXC35CV1B","FTXC50CV1B / RXC50CV1B","FTXC60CV1B / RXC60CV1B","FTXC71CV1B / RXC71CV1B"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.3","1.3","1.4","1.8","2.3"]
["","Maks.","","kW","3.0","3.0","4.0","6.2","7.0","7.3"]
["Hlađenje prostora","SEER","","","6.89","6.84","6.87","6.45","6.40","5.30"]
["","Godišnja potrošnja električne energije","","kWh/god.","106","132","175","276","340","459"]
["","Kapacitet","Pdesign","kW","2.08","2.57","3.44","5.08","6.21","6.96"]
["","Klasa energetske efikasnosti","","","A++","A++","A++","A++","A++","A"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","1.87","2.23","2.24","3.90","4.10","6.35"]
["","SCOP/A","","","4.40","4.45","4.28","4.42","4.24","3.81"]
["","Klasa energetske efikasnosti","","","A+","A+","A+","A+","A+","A"]
["","Godišnja potrošnja električne energije","","kWh/god.","594","700","732","1,236","1,354","2,334"]
["Nominalna efikasnost","EER","","","3.36","3.35","3.35","3.29","3.30","2.98"]
["","COP","","","3.73","3.79","3.74","3.71","3.81","3.25"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A","A","A","C"]
["","","Grejanje","","A","A","A","A","A","C"]
["Kapacitet grejanja","Min.","","kW","1.30","1.30","1.30","1.36","1.48","2.30"]
["","Maks.","","kW","4.00","4.00","4.80","6.60","8.00","9.00"]