{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AW9 / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BW9 / RXJ20M5V1B9","FTXJ25A2V1BW9 / RXJ25M5V1B9","FTXJ35A2V1BW9  / RXJ35M5V1B9","FTXJ35A2V1BW9 / RXJ35M5V1B9"]
["Kapacitet hlađenja","Nom.","","kW","2.30","2.40","3.50","3.50"]
["Kapacitet grejanja","Nom.","","kW","2.50","3.20","4.00","4.00"]
["Nominalna efikasnost","EER","","","4.64","4.73","4.09","4.09"]
["","COP","","","5.00","4.57","4.04","4.04"]
["","Godišnja potrošnja električne energije","","kWh","248","254","428","428"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A","A"]
["","","Grejanje","","A","A","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+++","A+++","A++","A++"]
["","Kapacitet","Pdesign","kW","2.30","2.40","3.50","3.50"]
["","SEER","","","8.73","8.64","7.19","7.19"]
["","Godišnja potrošnja električne energije","","kWh/a","92","97","170","170"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","2.10","2.70","3.00","3.00"]
["","SCOP/A","","","4.61","4.60","4.60","4.60"]
["","Pdh Kapacitet grejanja na -10°C","","kW","1.80","2.18","2.61","2.61"]
["","Godišnja potrošnja električne energije","","kWh/a","638","822","913","913"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]