{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Grejanje","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Kućište","Boja","","","","Bela","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","303","303","303","303"]
["","","","Širina","mm","998","998","998","998"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","212","212","212","212"]
["Težina","Uređaj","","","kg","12","12","12","12"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","8.9","8.9","10.9","10.9"]
["","","","Srednji","m³/min","6.6","6.6","7.8","8.9"]
["","","","Nizak","m³/min","4.4","4.4","4.8","6.8"]
["","","","Nečujan rad","m³/min","2.6","2.6","2.9","3.6"]
["","","Grejanje","Visok","m³/min","10.2","11.0","12.4","12.6"]
["","","","Srednji","m³/min","8.4","8.6","9.6","10.5"]
["","","","Nizak","m³/min","6.3","6.3","6.9","8.1"]
["","","","Nečujan rad","m³/min","3.8","3.8","4.1","5.0"]
["Nivo zvučne snage","Hlađenje","","","dBA","54","54","59","60"]
["","Grejanje","","","dBA","56","56","59","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","38","38","45","46"]
["","","","Srednji","dBA","32","32","34","40"]
["","","","Nizak","dBA","25","25","26","35"]
["","","","Nečujan rad","dBA","19","19","20","25"]
["","Grejanje","","Visok","dBA","40","41","45","47"]
["","","","Srednji","dBA","34","34","37","41"]
["","","","Nizak","dBA","28","28","29","35"]
["","","","Nečujan rad","dBA","19","19","20","25"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.50","9.50","9.50","12.70"]
["","Ispusni otvor","","","","18","18","18","18"]
["Control systems","Infracrveni daljinski upravljač","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Napajanje","Ime","","","","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Beleške","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]