{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 4MWXM-A"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / FTXM25R2V1B / 4MWXM52A2V1B","FTXM25R5V1B / FTXM25R5V1B / 4MWXM52A2V1B"]
["Kapacitet hlađenja","Nom.","","kW","5.00","5.00"]
["Kapacitet grejanja","Nom.","","kW","6.80","6.80"]
["Nominalna efikasnost","EER","","","4.85","4.85"]
["","COP","","","4.45","4.45"]
["","Godišnja potrošnja električne energije","","kWh","515","515"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","5.00","5.00"]
["","SEER","","","8.59","8.59"]
["","Godišnja potrošnja električne energije","","kWh/god.","204","204"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A+","A+"]
["","Kapacitet","Pdesign","kW","4.80","4.80"]
["","SCOP/A","","","4.38","4.38"]
["","Pdh Kapacitet grejanja na -10°C","","kW","3.82","3.82"]
["","Godišnja potrošnja električne energije","","kWh/god.","1533","1533"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]