{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":18,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-N9"]
[]
[]
[]
[]
["","","","","FTXM20R2V1B / RXM20N5V1B9","FTXM20R5V1B / RXM20N5V1B9","FTXM20R2V1B / RXM20N2V1B9","FTXM25R2V1B / RXM25N5V1B9","FTXM25R5V1B / RXM25N5V1B9","FTXM20R5V1B / RXM20N2V1B9","FTXM25R2V1B / RXM25N2V1B9","FTXM25R5V1B / RXM25N2V1B9","FTXM35R5V1B / RXM35N5V1B9","FTXM35R2V1B / RXM35N5V1B9","FTXM35R2V1B / RXM35N2V1B9","FTXM35R5V1B / RXM35N2V1B9","FTXM50R2V1B / RXM50N2V1B9","FTXM60R2V1B / RXM60N2V1B9"]
["Spoljni uređaj","","","","RXM20N5V1B9","RXM20N5V1B9","RXM20N5V1B9","RXM25N5V1B9","RXM25N5V1B9","RXM20N5V1B9","RXM25N5V1B9","RXM25N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM50N2V1B9","RXM60N2V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.30","1.30","","1.30","1.30","","","","1.40","1.40","","","1.70","1.70"]
["","Nom.","","kW","2.00","2.00","","2.50","2.50","","","","3.40","3.40","","","5.00","6.00"]
["","Maks.","","kW","2.60","2.60","","3.20","3.20","","","","4.00","4.00","","","6.00","7.00"]
["Kapacitet grejanja","Min.","","kW","1.30","1.30","","1.30","1.30","","","","1.40","1.40","","","1.70","1.70"]
["","Nom.","","kW","2.50","2.50","","2.80","2.80","","","","4.00","4.00","","","5.80","7.00"]
["","Maks.","","kW","3.50","3.50","","4.70","4.70","","","","5.20","5.20","","","7.70","8.00"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","219","219","","278","278","","","","402","402","","","679","885"]
["","COP","","","5.00","5.00","","5.00","5.00","","","","4.04","4.04","","","4.00","3.61"]
["","EER","","","4.57","4.57","","4.50","4.50","","","","4.23","4.23","","","3.68","3.39"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","","A","A","","","","A","A","","","A","A"]
["","","Grejanje","","A","A","","A","A","","","","A","A","","","A","A"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Kapacitet hlađenja","Min.","","kW","","","1.30","","","1.30","1.30","1.30","","","1.40","1.40"]
["","Nom.","","kW","","","2.00","","","2.00","2.50","2.50","","","3.40","3.40"]
["","Maks.","","kW","","","2.60","","","2.60","3.20","3.20","","","4.00","4.00"]
["Kapacitet grejanja","Min.","","kW","","","1.30","","","1.30","1.30","1.30","","","1.40","1.40"]
["","Nom.","","kW","","","2.50","","","2.50","2.80","2.80","","","4.00","4.00"]
["","Maks.","","kW","","","3.50","","","3.50","4.70","4.70","","","5.20","5.20"]
["Nominalna efikasnost","EER","","","","","4.57","","","4.57","4.50","4.50","","","4.23","4.23"]
["","COP","","","","","5.00","","","5.00","5.00","5.00","","","4.04","4.04"]
["","Godišnja potrošnja električne energije","","kWh","","","219","","","219","278","278","","","402","402"]
["","Direktiva o energetskom označavanju","Hlađenje","","","","A","","","A","A","A","","","A","A"]
["","","Grejanje","","","","A","","","A","A","A","","","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","","A+++","","","A+++","A+++","A+++","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","","","2.00","","","2.00","2.50","2.50","","","3.40","3.40"]
["","SEER","","","","","8.65","","","8.65","8.65","8.65","","","8.65","8.65"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","81","","","81","101","101","","","138","138"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","","A+++","","","A+++","A+++","A+++","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","","","2.30","","","2.30","2.40","2.40","","","2.50","2.50"]
["","SCOP/A","","","","","5.10","","","5.10","5.10","5.10","","","5.10","5.10"]
["","Pdh Kapacitet grejanja na -10°C","","kW","","","2.24","","","2.24","2.30","2.30","","","2.35","2.35"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","632","","","632","659","659","","","687","687"]
["Opseg energetske efikasnosti","","","","","","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]