{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-R9"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / RXM20R5V1B9","FTXM20R2V1B / RXM20R5V1B9","FTXM25R5V1B / RXM25R5V1B9","FTXM25R2V1B / RXM25R5V1B9","FTXM35R5V1B / RXM35R5V1B9","FTXM35R2V1B / RXM35R5V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.30","","1.30","","1.40"]
["","Nom.","","kW","2.00","","2.50","","3.40"]
["","Maks.","","kW","2.60","","3.20","","4.00"]
["Kapacitet grejanja","Min.","","kW","1.30","","1.30","","1.40"]
["","Nom.","","kW","2.50","","2.80","","4.00"]
["","Maks.","","kW","3.50","","4.70","","5.20"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","219","","278","","402"]
["","COP","","","5.00","","5.00","","4.04"]
["","EER","","","4.57","","4.50","","4.23"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","","A","","A"]
["","","Grejanje","","A","","A","","A"]
["Beleške","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","(3) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(3) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(4) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["Kapacitet hlađenja","Min.","","kW","","1.3","","1.3","","1.4"]
["","Nom.","","kW","","2","","2.5","","3.4"]
["","Maks.","","kW","","2.6","","3.2","","4"]
["Kapacitet grejanja","Min.","","kW","","1.3","","1.3","","1.4"]
["","Nom.","","kW","","2.5","","2.8","","4"]
["","Maks.","","kW","","3.5","","4.7","","5.2"]
["Nominalna efikasnost","EER","","","","4.57","","4.5","","4.23"]
["","COP","","","","5","","5","","4.04"]
["","Godišnja potrošnja električne energije","","kWh","","219","","278","","402"]
["","Direktiva o energetskom označavanju","Hlađenje","","","A","","A","","A"]
["","","Grejanje","","","A","","A","","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","","A+++","","A+++","","A+++"]
["","Kapacitet","Pdesign","kW","","2","","2.5","","3.4"]
["","SEER","","","","8.65","","8.65","","8.65"]
["","Godišnja potrošnja električne energije","","kWh/a","","81","","101","","137"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","","A+++","","A+++","","A+++"]
["","Kapacitet","Pdesign","kW","","2.3","","2.4","","2.5"]
["","SCOP/A","","","","5.1","","5.1","","5.1"]
["","Pdh Kapacitet grejanja na -10°C","","kW","","2.24","","2.3","","2.35"]
["","Godišnja potrošnja električne energije","","kWh/a","","631","","659","","686"]