{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M"]
[]
[]
[]
[]
["","","","","","FTXP20M5V1B","FTXP25M5V1B","FTXP35M5V1B","FTXP50M2V1B","FTXP60M2V1B","FTXP71M2V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.019","0.02","0.032","0.029","0.032","0.032"]
["","Grejanje","","Nom.","kW","0.023","0.023","0.032","0.032","0.035","0.035"]
["Kućište","Boja","","","","Bela","Bela","Bela","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286","295","295","295"]
["","","","Širina","mm","770","770","770","990","990","990"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","225","225","225","263","263","263"]
["Težina","Uređaj","","","kg","8.5","8.5","9","13.5","13.5","13.5"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","9.5","9.7","11.5","16.3","16.8","16.8"]
["","","","Srednji","m³/min","7.4","7.7","8.3","14","14.4","14.4"]
["","","","Nizak","m³/min","5.6","5.8","6.3","11.5","11.8","11.8"]
["","","","Nečujan rad","m³/min","4.2","4.2","4.5","8.3","9.2","10.1"]
["","","Grejanje","Visok","m³/min","10.4","10.4","11.5","17.3","17.9","17.9"]
["","","","Srednji","m³/min","8.1","8.1","9","14.4","15.3","15.3"]
["","","","Nizak","m³/min","6.2","6.4","7","11.8","12.4","12.4"]
["","","","Nečujan rad","m³/min","5.2","5.2","5.3","10.4","11","11"]
["Nivo zvučne snage","Hlađenje","","","dBA","55","55","58","59","60","62"]
["","Grejanje","","","dBA","55","55","58","61","62","62"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","39","40","43","43","45","46"]
["","","","Srednji","dBA","33","33","34","39","41","42"]
["","","","Nizak","dBA","25","26","27","34","36","37"]
["","","","Nečujan rad","dBA","19","19","20","27","30","32"]
["","Grejanje","","Visok","dBA","39","40","40","42","44","45"]
["","","","Srednji","dBA","34","34","35","38","40","41"]
["","","","Nizak","dBA","28","28","29","33","35","36"]
["","","","Nečujan rad","dBA","21","21","21","30","32","33"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.5","9.5","9.5","12.7","12.7","12.7"]
["","Ispusni otvor","","","","18","18","18","18","18","18"]
["Kontrolni sistemi","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53","ARC480A53","ARC480A53","ARC480A53"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardni pribor","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2","1","1","1"]
["","Silver particle filter","","","","1","","","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Napajanje","Ime","","","","","","","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]