{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Spoljni uređaj","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Kapacitet hlađenja","Min.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Maks.","","kW","","3.0"]
["Kapacitet grejanja","Min.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Maks.","","kW","","4.00"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Direktiva o energetskom označavanju","Hlađenje","","","A"]
["","","Grejanje","","","A"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Kapacitet hlađenja","Min.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Maks.","","kW","2.6","","4.0"]
["Kapacitet grejanja","Min.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Maks.","","kW","3.50","","4.80"]
["Nominalna efikasnost","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Godišnja potrošnja električne energije","","kWh","249"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","","A"]
["","","Grejanje","","A","","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Godišnja potrošnja električne energije","","kWh/god.","103","","186"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","","A++"]
["","Kapacitet","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Pdh Kapacitet grejanja na -10°C","","kW","1.99","","2.33"]
["","Godišnja potrošnja električne energije","","kWh/god.","662","","845"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","","A+++ ~ D"]