{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9 / RXP-N9"]
[]
[]
[]
[]
["","","","","FTXP20N5V1B9 / RXP20N5V1B9","FTXP25N5V1B9 / RXP25N5V1B9","FTXP35N5V1B9 / RXP35N5V1B9"]
["Outdoor unit","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2","2.5","3.5"]
["","Maks.","","kW","2.6","3","4"]
["Kapacitet grejanja","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.5","3","4"]
["","Maks.","","kW","3.5","4","4.8"]
["Nominalna efikasnost","EER","","","3.75","3.75","3.48"]
["","COP","","","4.77","4.36","4.02"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A"]
["","","Grejanje","","A","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","2","2.5","3.5"]
["","SEER","","","7.2","7.2","7.2"]
["","Godišnja potrošnja električne energije","","kWh/god.","97","121","170"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","2.2","2.4","2.8"]
["","SCOP/A","","","4.65","4.61","4.64"]
["","Pdh Kapacitet grejanja na -10°C","","kW","1.99","2.09","2.35"]
["","Godišnja potrošnja električne energije","","kWh/god.","663","728","845"]
["Beleške","","","","(1) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(1) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(1) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(2) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(2) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(2) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]