{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9"]
[]
[]
[]
[]
["","","","","","FTXP25N5V1B9","FTXP35N5V1B9","FTXP50N5V1B9","FTXP20N5V1B9 (Archived)"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.023","0.032","0.04","0.021"]
["","Grejanje","","Nom.","kW","0.023","0.032","0.04","0.023"]
["Kućište","Boja","","","","Bela","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","286","286","286","286"]
["","","","Širina","mm","770","770","770","770"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","225","225","225","225"]
["Težina","Uređaj","","","kg","9","9","9","9"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","9.9","11.5","11.8","9.6"]
["","","","Srednji","m³/min","7.5","8.3","9.3","7.5"]
["","","","Nizak","m³/min","5.8","6.3","7.6","5.6"]
["","","","Nečujan rad","m³/min","4.4","4.5","6","4.4"]
["","","Grejanje","Visok","m³/min","10.6","11.5","11.9","10.6"]
["","","","Srednji","m³/min","8.6","9","9.5","8.6"]
["","","","Nizak","m³/min","6.6","7","8.2","6.6"]
["","","","Nečujan rad","m³/min","5","5.1","7.4","5"]
["Nivo zvučne snage","Hlađenje","","","dBA","55","58","59","55"]
["","Grejanje","","","dBA","55","58","61","55"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","40","43","46","39"]
["","","","Srednji","dBA","33","34","39","33"]
["","","","Nizak","dBA","26","27","34","25"]
["","","","Nečujan rad","dBA","19","20","27","19"]
["","Grejanje","","Visok","dBA","40","40","44","39"]
["","","","Srednji","dBA","34","35","38","34"]
["","","","Nizak","dBA","28","29","33","28"]
["","","","Nečujan rad","dBA","21","21","30","21"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.52","9.52","12.7","9.52"]
["","Ispusni otvor","","","","18","18","18","18"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC480A78","ARC480A78","ARC480A78","ARC480A78"]
["","Žičani daljinski upravljač","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB; odgovarajuća dužina cevi: 5 m; visinska razlika: 0m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m (po horizontali)"]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]