{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-K"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20K2V1B","FTXS20K2V1B / RXS20K3V1B","FTXS25K2V1B / RXS25K2V1B","FTXS25K2V1B / RXS25K3V1B","FTXS35K2V1B / RXS35K2V1B","FTXS42K2V1B / RXS42K2V1B","FTXS50K2V1B / RXS50K2V1B"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.3","1.3","1.3","1.4","1.7","1.7"]
["","Maks.","","kW","2.8","2.8","3.2","3.2","4.0","5.0","5.3"]
["","Nom.","","kW","2.0 (3)","2.0 (2)","2.5 (3)","2.5 (2)","3.50 (2)","4.20 (2)","5.00 (2)"]
["Povezivanje cevi","Tečnost","SP","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Ispusni otvor","OD","mm","18.0","18.0","18.0","18.0","18","18","18"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","215","215","285","285","420","590","705"]
["","EER","","","4.65","4.65","4.39","4.39","4.17","3.56","3.55"]
["","COP","","","4.55","4.55","4.52","4.52","4.76","4.12","4.00"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A","A","A","A","A"]
["","","Grejanje","","A","A","A","A","A","A","A"]
["Kapacitet grejanja","Nom.","","kW","2.5 (4)","2.5 (3)","2.8 (4)","2.8 (3)","4.00 (3)","5.40 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.4","1.7","1.7"]
["","Maks.","","kW","4.3","4.3","4.7","4.7","5.2","6.0","6.5"]
["Beleške","","","","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - Energetska oznaka: skala od A (najefikasnije) do G (najmanja efikasnost)","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5m","(2) - Godišnja potrošnja energije: na osnovi prosečne upotrebe od 500 radnih časova godišnje pod punim opterećenjem (nominalni uslovi)","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB; odgovarajuća dužina cevi: 5m","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(2) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","(3) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(3) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(3) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(4) - 220V","(4) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(4) - 220V","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - 220V","(5) - 230V","(5) - 220V","(5) - 230V","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","(6) - 230V","(6) - 240V","(6) - 230V","(6) - 240V","(6) - 240V","(6) - 240V","(6) - 240V"]
["","","","","(7) - 240V","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(7) - 240V","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(7) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]
["","","","","(8) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","","(8) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]