{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","40","","","","","","45"]
["","","","Nečujan rad","dBA","19","","","","","","22"]
["","","","Nizak","dBA","27","","","","","","33"]
["","Hlađenje","","Nečujan rad","dBA","19","","","","","","21"]
["","","","Nizak","dBA","24","","","","","","33"]
["","","","Visok","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Hlađenje","","Nom.","dBA","32","","","","","","39"]
["Standardni pribor","Priručnik za instalaciju","","","","1","","","","","","1"]
["","Priručnik za upotrebu","","","","1","","","","","","1"]
["","Bežični daljinski upravljač","","","","1","","","","","","1"]
["","Baterije","","","","2","","","","","","2"]
["","Držač daljinskog upravljača","","","","1","","","","","","1"]
["","Noseća ploča","","","","1","","","","","","1"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","","2","","","","","","2"]
["","Fotokatalitički filter za vazduh od titanijumapatita","","","","2","","","","","","2"]
["Kontrolni sistemi","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Cevne spojnice","Tečnost","","SP","mm","6.35","","","","","","6.35"]
["","Gas","","SP","mm","9.5","","","","","","9.5"]
["","Ispusni otvor","","","","18","","","","","","18"]
["Apsorbovana snaga","Hlađenje","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grejanje","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Hlađenje","","","dBA","58","","","","","","59"]
["","Grejanje","","","dBA","58","","","","","","59"]
["Dimenzije","Uređaj","","Širina","mm","780","","","","","","900"]
["","","","Dubina","mm","215","","","","","","215"]
["","","","Visina","mm","289","","","","","","298"]
["Kućište","Boja","","","","Bela","","","","","","Bela"]
["Težina","Uređaj","","","kg","8","","","","","","11"]
["Power supply","Faza","","","","1~","","","","","","1~"]
["","Frekvencija","","","Hz","50","","","","","","50"]
["","Ime","","","","V1","","","","","","V1"]
["","Napon","","","V","220-240","","","","","","220-240"]
["Beleške","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Grejanje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Kućište","Boja","","","","","Bela","Bela","Bela","Bela","Bela","","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","","215","289","215","298","215","","215","298","215"]
["","","","Širina","mm","","780","780","780","900","900","","900","900","900"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","289","215","289","215","298","","298","215","298"]
["Težina","Uređaj","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Srednji","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Nizak","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Nečujan rad","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Grejanje","Visok","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Srednji","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Nizak","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Nečujan rad","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Grejanje","","","dBA","","58","58","58","59","59","","59","60","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Srednji","dBA","","32","33","33","","37","","39","","40"]
["","","","Nizak","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Nečujan rad","dBA","","19","19","19","19","19","","21","23","23"]
["","Grejanje","","Visok","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Srednji","dBA","","34","34","34","","39","","39","","40"]
["","","","Nizak","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Nečujan rad","dBA","","19","19","19","19","19","","22","24","24"]
["Povezivanje cevi","Tečnost","","SP","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","SP","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Ispusni otvor","","","","","18","18","18","18","18","","18","18","18"]
["Kontrolni sistemi","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardni pribor","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Napajanje","Ime","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napon","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Brzina protoka vazduha","Grejanje","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Nivo zvučnog pritiska","Grejanje","","Nom.","dBA","","","34","","39","","","","40"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardni pribor","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Beleške","","","","","","","","","","","(4) - 240V"]