{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.029","0.053"]
["","Grejanje","","Nom.","kW","0.024","0.06"]
["Kućište","Boja","","","","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","298","298"]
["","","","Širina","mm","804","997"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","252","292"]
["Težina","Uređaj","","","kg","12","15"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","13.2","15.1"]
["","","","Srednji","m³/min","8.1","9.2"]
["","","","Nizak","m³/min","5.6","5.6"]
["","","","Nečujan rad","m³/min","4.8","4.8"]
["","","Grejanje","Visok","m³/min","11.7","17"]
["","","","Srednji","m³/min","7.7","10"]
["","","","Nizak","m³/min","5.6","6"]
["","","","Nečujan rad","m³/min","4.7","5.1"]
["Nivo zvučne snage","Hlađenje","","","dBA","60","60"]
["","Grejanje","","","dBA","59","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","45","46"]
["","","","Srednji","dBA","33","32"]
["","","","Nizak","dBA","25","24"]
["","","","Nečujan rad","dBA","21","20"]
["","Grejanje","","Visok","dBA","43","46"]
["","","","Srednji","dBA","31","31"]
["","","","Nizak","dBA","22","22"]
["","","","Nečujan rad","dBA","19","19"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","675","675"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35"]
["","Gas","","SP","mm","9.5","9.5"]
["","Ispusni otvor","","","","18","18"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC466A83","ARC466A83"]
["Standardni pribor","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Ime","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Standardni pribor","FTXTM40A2V1B","","","","","1"]