{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30R2V1B / RXTM30A2V1B","FTXTM40R2V1B / RXTM40A2V1B"]
["Kapacitet hlađenja","Min.","","kW","0.70","0.90"]
["","Nom.","","kW","3.00","4.00"]
["","Maks.","","kW","4.50","5.10"]
["Kapacitet grejanja","Min.","","kW","0.80","1.20"]
["","Nom.","","kW","3.20","4.00"]
["","Maks.","","kW","6.70","7.20"]
["Nominalna efikasnost","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Godišnja potrošnja električne energije","","kWh","366","539"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A"]
["","","Grejanje","","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A++","A++"]
["","Kapacitet","Pdesign","kW","3.00","4.00"]
["","SEER","","","7.60","7.70"]
["","Godišnja potrošnja električne energije","","kWh/god.","138","182"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","3.00","3.80"]
["","SCOP/A","","","5.12","5.30"]
["","Pdh Kapacitet grejanja na -10°C","","kW","3.00","3.80"]
["","Godišnja potrošnja električne energije","","kWh/god.","821","1003"]