{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","45.0"]
["","","","Srednji","dBA","31.0"]
["","","","Nečujan rad","dBA","19.0"]
["","","","Nizak","dBA","22.0"]
["","Hlađenje","","Medium","dBA","33.0"]
["","","","Nečujan rad","dBA","21.0"]
["","","","Nizak","dBA","25.0"]
["","","","Visok","dBA","45.0"]
["Standardni pribor","Priručnik za instalaciju","","","","1"]
["","Priručnik za upotrebu","","","","1"]
["","Bežični daljinski upravljač","","","","1"]
["","AAA suve baterije","","","","2"]
["","Držač daljinskog upravljača","","","","1"]
["","Noseća ploča","","","","1"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","","2"]
["","Srebrni filter za prašinu","","","","1"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35"]
["","Gas","","SP","mm","9.50"]
["","Ispusni otvor","","","","18"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.035"]
["","Grejanje","","Nom.","kW","0.039"]
["Sound power level","Hlađenje","","","dBA","60.0"]
["","Grejanje","","","dBA","61.0"]
["Dimenzije","Uređaj","","Širina","mm","778"]
["","","","Dubina","mm","272"]
["","","","Visina","mm","295"]
["Kućište","Boja","","","","Bela"]
["Težina","Uređaj","","","kg","10.0"]
["Ventilator","Brzina protoka vazduha","Grejanje","Visok","m³/min","12.5"]
["","","","Nizak","m³/min","4.9"]
["","","","Medium","m³/min","7.5"]
["","","","Nečujan rad","m³/min","4.0"]
["","","Hlađenje","Nizak","m³/min","5.3"]
["","","","Medium","m³/min","7.8"]
["","","","Visok","m³/min","12.2"]
["","","","Nečujan rad","m³/min","4.1"]
["Power supply","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Ime","","","","V1"]
["","Napon","","","V","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27 °CDB, 19.0 °CWB; spoljnoj temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","0.053"]
["","Grejanje","","Nom.","kW","","0.06"]
["Kućište","Boja","","","","","Bela"]
["Dimenzije","Uređaj","","Visina","mm","","299"]
["","","","Širina","mm","","998"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","292"]
["Težina","Uređaj","","","kg","","14.5"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","15.4"]
["","","","Srednji","m³/min","","9.5"]
["","","","Nizak","m³/min","","5.8"]
["","","","Nečujan rad","m³/min","","4.6"]
["","","Grejanje","Visok","m³/min","","17.5"]
["","","","Srednji","m³/min","","10.5"]
["","","","Nizak","m³/min","","7.1"]
["","","","Nečujan rad","m³/min","","5.9"]
["Nivo zvučne snage","Hlađenje","","","dBA","","60"]
["","Grejanje","","","dBA","","61"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","46"]
["","","","Srednji","dBA","","32"]
["","","","Nizak","dBA","","24"]
["","","","Nečujan rad","dBA","","20"]
["","Grejanje","","Visok","dBA","","46"]
["","","","Srednji","dBA","","31"]
["","","","Nizak","dBA","","22"]
["","","","Nečujan rad","dBA","","19"]
["Povezivanje cevi","Tečnost","","SP","mm","","6.35"]
["","Gas","","SP","mm","","9.5"]
["","Ispusni otvor","","","","","18"]
["Kontrolni sistemi","Infrared remote control","","","","","ARC466A75"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","","BRC073A1"]
["Standardni pribor","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napajanje","Ime","","","","","V1"]
["","Faza","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]