{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.035","0.053"]
["","Grejanje","","Nom.","kW","0.039","0.06"]
["Kućište","Boja","","","","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","295","299"]
["","","","Širina","mm","778","998"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","272","292"]
["Težina","Uređaj","","","kg","10","15"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","11.5","15.1"]
["","","","Srednji","m³/min","7.5","9.2"]
["","","","Nizak","m³/min","5.2","5.6"]
["","","","Nečujan rad","m³/min","4.2","4.8"]
["","","Grejanje","Visok","m³/min","11.6","17"]
["","","","Srednji","m³/min","7.3","10"]
["","","","Nizak","m³/min","4.7","6"]
["","","","Nečujan rad","m³/min","4","5.1"]
["Nivo zvučne snage","Hlađenje","","","dBA","60","60"]
["","Grejanje","","","dBA","60","60"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","45","46"]
["","","","Srednji","dBA","33","32"]
["","","","Nizak","dBA","25","24"]
["","","","Nečujan rad","dBA","21","20"]
["","Grejanje","","Visok","dBA","45","46"]
["","","","Srednji","dBA","31","31"]
["","","","Nizak","dBA","22","22"]
["","","","Nečujan rad","dBA","19","19"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","675","675"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35"]
["","Gas","","SP","mm","9.5","9.5"]
["","Ispusni otvor","","","","18","18"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC466A83","ARC466A83"]
["","Žičani daljinski upravljač","","","","BRC073A1","BRC073A1"]
["Standardni pribor","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]