{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","43"]
["","","","Srednji","dBA","35"]
["","","","Nečujan rad","dBA","21"]
["","","","Nizak","dBA","26"]
["","Hlađenje","","Srednji","dBA","35"]
["","","","Nečujan rad","dBA","21"]
["","","","Nizak","dBA","26"]
["","","","Visok","dBA","43"]
["Standardni pribor","Priručnik za instalaciju","","","","1"]
["","Priručnik za upotrebu","","","","1"]
["","Bežični daljinski upravljač","","","","1"]
["","AAA suve baterije","","","","2"]
["","Držač daljinskog upravljača","","","","1"]
["","Noseća ploča","","","","1"]
["","Titanijumapatitski dezodorišući filter","","","","2"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","","2"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35"]
["","Gas","","SP","mm","9.50"]
["","Ispusni otvor","","","","16 (unutrašnji prečnik priključne cevi)"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.030"]
["","Grejanje","","Nom.","kW","0.035"]
["Nivo zvučne snage","Hlađenje","","","dBA","58"]
["","Grejanje","","","dBA","58"]
["Dimenzije","Uređaj","","Širina","mm","770"]
["","","","Dubina","mm","225"]
["","","","Visina","mm","285"]
["Kućište","Boja","","","","Bela"]
["Težina","Uređaj","","","kg","9.0"]
["Power supply","Faza","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Ime","","","","V1"]
["","Napon","","","V","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Ulazna snaga","Hlađenje","","Nom.","kW","","0.03"]
["","Grejanje","","Nom.","kW","","0.035"]
["Kućište","Boja","","","","","Bela"]
["Dimenzije","Uređaj","","Visina","mm","","285"]
["","","","Širina","mm","","770"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","225"]
["Težina","Uređaj","","","kg","","9"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","","11.4"]
["","","","Srednji","m³/min","","8.2"]
["","","","Nizak","m³/min","","5.4"]
["","","","Nečujan rad","m³/min","","4.3"]
["","","Grejanje","Visok","m³/min","","10.8"]
["","","","Srednji","m³/min","","7.8"]
["","","","Nizak","m³/min","","5.8"]
["","","","Nečujan rad","m³/min","","4.9"]
["Nivo zvučne snage","Hlađenje","","","dBA","","58"]
["","Grejanje","","","dBA","","58"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","43"]
["","","","Srednji","dBA","","35"]
["","","","Nizak","dBA","","26"]
["","","","Nečujan rad","dBA","","21"]
["","Grejanje","","Visok","dBA","","43"]
["","","","Srednji","dBA","","35"]
["","","","Nizak","dBA","","26"]
["","","","Nečujan rad","dBA","","21"]
["Povezivanje cevi","Tečnost","","SP","mm","","6.35"]
["","Gas","","SP","mm","","9.5"]
["","Ispusni otvor","","","","","16 (unutrašnji prečnik priključne cevi)"]
["Kontrolni sistemi","Infrared remote control","","","","","ARC480A11"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","","BRC944B2, BRC073A1"]
["Standardni pribor","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napajanje","Ime","","","","","V1"]
["","Faza","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50"]
["","Napon","","","V","","220-240"]